**Installing OpenCV for Webots (Windows Only)**

**Jeffrey Cheng and Victor Hu**

1. Go to <https://github.com/huihut/OpenCV-MinGW-Build> and download the zip for OpenCV 4.1.1 (or whatever version you want to use)

A screenshot of a cell phone

Description automatically generated

1. Open the zip and extract the contents into your C:\ drive

A screenshot of a social media post

Description automatically generated

A screenshot of a social media post

Description automatically generated

1. Separately, search “path” into the Windows search bar and hit enter (should bring up Edit the system environment variables)

A screenshot of a cell phone

Description automatically generated

1. Click on Environment Variables and an “Environment Variables” window should appear

A screenshot of a social media post

Description automatically generated

1. A screenshot of a social media post

   Description automatically generatedClick on Path and press Edit, and a “Edit environment variable” window should appear
2. Switch back to your C:\ drive and navigate the following path

A screenshot of a cell phone

Description automatically generated

1. Copy the path by clicking directly to the right of “bin” and pressing ctrl c - the path should be “C:\OpenCV-MinGW-Build-OpenCV-4.1.1-x64\x64\mingw\bin” if you followed the steps exactly

A screenshot of a computer

Description automatically generated

1. Switch back to the “Edit environment variable” window from before, press new, paste in the folder path you copied from before

A screenshot of a computer

Description automatically generated

1. You can now press “OK” on all windows until all of them disappear. You have now successfully downloaded the pre-built OpenCV library for Windows and added it to a list of paths that search for libraries. Now, we have to create a Webots robot controller that can find its way to the OpenCV folder. Create a new robot controller like normal by going to Wizards -> New Robot Controller, and following the steps.

A screenshot of a computer screen

Description automatically generated

1. Separately, navigate to the folder that your world is stored in, go up one level, go into the folder named “controllers,” and enter the folder that has the same name as your robot controller.

A screenshot of a computer

Description automatically generated

1. Edit the Makefile with a text editor of your choosing – I am using Notepad++

A screenshot of a computer

Description automatically generated

1. Go to our GitHub page -> Day3 and open Makefile (or use this link: <https://github.com/victorhu3/Webots-Sample-Code/blob/master/Day3/Makefile>). Then, copy lines 50 and 51.

A screenshot of a social media post

Description automatically generated

1. Go back to the Makefile that you opened with your chosen text editor and replace that Makefile’s lines 50 and 51 with the two lines that you just copied.

A screenshot of a computer

Description automatically generated

1. Save the Makefile, and now you are free to use the OpenCV library in the robot controller that you just created!